{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":79,"n_cols":2,"rows_kept":79,"merged":[[0,0,0,1],[1,0,1,1]]}
["The supply of High-Performance Computing Platform to the CSIR  "]
[" RFP No: 3492/10/12/2021"]
["Functional requirment","weight %"]
[]
[]
["Power and space efficiency of the of the total solution (Total Weight)",10]
["Solution area requirement total racks",5]
["Power consumption of the total solution Kw",5]
["sub total",{"$f":"SUM(B7:B8)","v":10}]
["Compute and network design and performance (Total Weight)",20]
["Reported sustained Linpack Rmax PF",10]
["Compute nodes RAM per x86 core",5]
["Interconnect bandwidth, latency, and expandability",5]
["sub total",{"$f":"SUM(B11:B13)","v":20}]
["System management software environment (Total Weight)",15]
["HPC Cluster Functional Features",10]
["                ·        Monitoring Metrics"]
["                ·        API"]
["                ·        Remote console"]
["                ·        Remote power control"]
["                ·        Smart PDUs"]
["                ·        CLI interface"]
["                ·        GUI interface"]
["                ·        Provisioning system"]
["                ·        Configuration Management system"]
["                ·        Version Control system"]
["                ·        Fault detection and Recovery system"]
["                ·        Access Control system"]
["                ·        Parallel shell"]
["                ·        High availability and failover for management and NFS servers"]
["NFS Backup",3]
["                ·        Usable capacity"]
["                ·        Incremental backup"]
["                ·        Automated backup"]
["                ·        Ransomware recovery"]
["Management nodes",2]
["                ·        Compliance with specification"]
["sub total",{"$f":"SUM(B16:B37)","v":15}]
["Integration with existing equipment (Total Weight)",10]
["NRE Storage",1]
["                ·        NRE users can login"]
["                ·        3PB Lustre can be accessed from the node"]
["                ·        Local storage can be accessed"]
["Fat Nodes",1]
["                ·        Users can execute jobs via the proposed scheduler"]
["                ·        The nodes can be monitored via the proposed monitoring solution"]
["                ·        The nodes can be managed via the proposed managment suite"]
["GPU Nodes",1]
["                ·        Users can execute jobs via the proposed scheduler"]
["                ·        The nodes can be monitored via the proposed monitoring solution"]
["                ·        The nodes can be managed via the proposed managment suite"]
["3PB Lustre",7]
["                ·        All nodes can mount 3PB Lustre"]
["                ·        Integration with the interconnect"]
["sub total",{"$f":"SUM(B40:B52)","v":10}]
["Partnership and HCD (Total Weight)",15]
["Student Cluster Competition (SCC) Sponsorship",2]
["Years of support/warranty (Duration and response time)",2]
["Onsite support staff (Number of staff and level of experience)",7]
["Training (Number of sessions and seats)",2]
["Mentorship/Exchange programme (Number and frequency)",2]
["sub total",{"$f":"SUM(B57:B61)","v":15}]
["Benchmarks (Total Weight)",30]
["Synthetic Benchmarks:"]
["HPCC1: HPL Rpeak [TFlop/s]",5]
["HPCC2: DGEMM [GFlop/s]",1]
["HPCC3: STREAM [GB/s]",1]
["HPCC4: PTRANS [GB/s]",1]
["HPCC5:RandomAccess [Giga updates /s]",1]
["HPCC6: FFT [GFlop/s]",1]
["HPCC7: Communication bandwidth [GB/s] and latency [μs]",3]
["HPCG [TFlop/s]",5]
["Application Benchmarks:"]
["(i) OpenFOAM [iters/s]",3]
["(ii) WRF [simulation hours per wallclock hour]",3]
["(iii) DL_Poly [MD Steps/sec]",3]
["(iv) Quantum_Espresso [runtime in h:m:s]",3]
["                sub total",{"$f":"SUM(B64:B77)","v":30}]
["Total Score",{"$f":"B78+B62+B55+B38+B14+B9","v":100}]