{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":2,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":57,"n_cols":23,"rows_kept":57,"merged":[[0,0,1,1],[0,2,1,2],[0,3,7,4],[0,5,7,9],[0,10,0,21],[0,22,7,22],[1,10,2,10],[1,11,2,12],[1,13,2,13],[1,14,2,14],[1,15,2,17],[1,18,1,21],[2,0,3,1],[2,2,3,2],[2,18,2,19],[2,20,2,21],[3,11,3,12],[3,15,3,17],[3,18,3,19],[3,20,3,21],[4,0,5,1],[4,2,5,2],[4,11,4,12],[4,15,4,17],[4,18,4,19],[4,20,4,21],[5,11,5,12],[5,15,5,17],[5,18,5,19],[5,20,5,21],[6,0,7,2],[6,11,6,12],[6,15,6,17],[6,18,6,19],[6,20,6,21],[7,11,7,12],[7,15,7,17],[7,18,7,19],[7,20,7,21],[8,0,10,0],[8,1,10,2],[8,3,10,3],[8,4,10,4],[8,5,10,5],[8,6,10,6],[8,7,10,7],[8,8,10,8],[8,9,8,11],[8,12,8,20],[8,21,10,21],[8,22,10,22],[9,9,10,9],[9,12,9,14],[9,15,9,17],[9,18,9,20],[11,0,11,22],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,0,15,22],[16,1,16,2],[17,1,17,2],[18,0,18,22],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,0,24,22],[25,1,25,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[29,0,29,22],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,0,33,22],[34,1,34,2],[35,1,35,2],[36,0,36,22],[37,1,37,2],[38,0,38,22],[39,1,39,2],[40,1,40,2],[41,0,41,22],[42,1,42,2],[43,1,43,2],[44,0,44,22],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[51,1,51,2]]}
["Project:",null,21050,{"$nulls":7},"Revision Status",{"$nulls":11},"Page 1 of 1"]
[{"$nulls":10},"Rev No.","Date",null,"Prepared By","Revised Sheet","Comments",null,null,"Approvals"]
["Document No.:",null,"21050-CSI-PR-LST-001",{"$nulls":15},"Checked  By",null,"Approved By "]
[{"$nulls":10},"A","11/08/2021",null,"YW","ALL","Issued for Internal Review",null,null,"JB",null,"JB"]
["Location:",null,"Glenwood, Durban",{"$nulls":7},"B","11/08/2021",null,"YW","ALL","Issued for Client Review",null,null,"JB",null,"JB"]
[{"$nulls":10},0,"16/08/2021",null,"YW","ALL","Issued for Information",null,null,"JB",null,"JB"]
["Battery Limit Schedule",{"$nulls":9},1,"02/09/2021",null,"JB","ALL","Issued for Information",null,null,"YW",null,"YW"]
[]
["No","Battery limit description",null,"Drawing No","Fluid State","Connection Type","Pipe Material","Nominal Size ","Wall  Thickness/ Schedule","Design condition",null,null,"Operating Condition",{"$nulls":8},"Tie-In No","Remarks"]
[{"$nulls":9},"Line class","Temperature (℃)","Pressure (kPa(g)) ","Flow",null,null,"Design Temperature (℃)",null,null,"Pressure (kPa(g))"]
[{"$nulls":10},"Min/Max","Min/Max ","Min","Normal","Max","Min","Normal","Max","Min","Normal","Max"]
["Parr Stirred Digestor"]
[1,"Main Water Supply",null,"21050-CSI-PR-PID-002","Liquid","Quick Fit","Poly urethane","6X4 mm","2 mm","-","5/40","0/1500","-","-","-","Ambient min","Ambient","Ambient Max",0,700,"900 kPa","TP-202"]
[2,"Nitrogen",null,"21050-CSI-PR-PID-002","Gas","MNPT","Braided Pipe (Stainless Steel)","3/8\"",null,"-","5/40","0/2500","-","-","-","Ambient min","Ambient","Ambient Max",0,600,"800 kPa","TP-203"]
[3,"Dry  Compressed Air",null,"21050-CSI-PR-PID-002","Gas","Quick Fit","Poly urethane","3/8\"","1.6mm","-","5/60","0/2500","-","-","-","Ambient min","Ambient",50,0,700,"800 kPa","TP-201"]
["Flow Through Digestor"]
[4,"Main Water Supply",null,"21050-CSI-PR-PID-003","Liquid","NPT Threaded Female","SS 316","1\"",null,"-","5/40","0/1500","-","-","-","Ambient min","Ambient","Ambient Max",0,700,"900 kPa","TP-204"]
[5,"Compressed Air",null,"21050-CSI-PR-PID-003","Gas","Quick Fit","Poly urethane","6X4 mm","2 mm","-","5/60","0/2500","-","-","-","Ambient min","Ambient",50,0,700,"800 kPa","TP-205"]
["RDH Digestor"]
[6,"Main Water Supply 1",null,"21050-CSI-PR-PID-004","Liquid","PN40 Flange","EN1.4404/316L","DN 20",null,"PN40","5/40","0/1500","0 LPM","5 LPM","15 LPM","Ambient min","Ambient","Ambient Max",400,600,800,"TP-212","To Process"]
[7,"Main Water Supply 2",null,"21050-CSI-PR-PID-004","Liquid","PN40 Flange","EN1.4404/316L","DN 20",null,"PN40","5/40","0/1500 ","0 LPM","20 LPM","30 LPM","Ambient min","Ambient","Ambient Max",300,500,600,"TP-211","To Coolers"]
[8,"Nitrogen",null,"21050-CSI-PR-PID-004","Gas","BSPP Socket","EN1.4404/316L","3/8\"",null,"-","5/40","0/2500","0 NL/min","5 NL/min","50 NL/min","Ambient min","Ambient","Ambient Max",1800,2000,2200,"TP-210"]
[9,"Compressed Air",null,"21050-CSI-PR-PID-004","Gas","BSPP Socket","EN1.4404/316L","3/8\"",null,"-","5/60","0/2500","0 NL/min","50 NL/min","200 NL/min","Ambient min","Ambient","Ambient Max",600,650,800,"TP-209"]
[10,"Steam",null,"21050-CSI-PR-PID-004","Gas","PN40 Flange","EN1.4404/316L","DN 20",null,"PN 40","0/220","Vaccum/2500","0 g/s","5 g/s","30 g/s",180,"190",200,1000,1200,1400,"TP-208"]
["Wastepaper Recycler"]
[11,"Main Water Supply",null,"21050-CSI-PR-PID-008","Liquid","Compression","Copper","15 mm",null,"Class 2","5/40","0/1500",0,"600 L/s","700 L/s","ambient","ambient","ambient",0,700,900,"TP-501A"]
[12,"Main Water Supply",null,"21050-CSI-PR-PID-008","Liquid","Compression","Copper","15 mm",null,"Class 2","5/40","0/1500",0,"600 L/s","700 L/s","ambient","ambient","ambient",0,700,900,"TP-501B"]
[13,"Main Water Supply",null,"21050-CSI-PR-PID-008","Liquid","Compression","Copper","15 mm",null,"Class 2","5/40","0/1500",0,"600 L/s","700 L/s","ambient","ambient","ambient",0,700,900,"TP-501C"]
[14,"Hot water",null,"21050-CSI-PR-PID-008","Liquid","Compression","Copper","15 mm",null,"Class 2","5/65","0/1500",0,"190 L/h\n0.05 L/s","*1.9 L/s\nDrainig from the 250 L",28,"50",60,0,300,400,"TP-502","\nHeat pump has an estimsated heat capapcity of 70l/h with an 4kW (120L/h) geyser, with a 250 L tank."]
["LC Refiner"]
[15,"Main Water Supply",null,"21050-CSI-PR-PID-009","Liquid","To Atmosphere","Copper","15 mm",null,"Class 2","5/40","0/1500",0,"600 L/s","700 L/s","ambient","ambient","ambient",0,700,900,"TP-503A"]
[16,"Main Water Supply",null,"21050-CSI-PR-PID-009","Liquid","To Atmosphere","Copper","15 mm",null,"Class 2","5/40","0/1500",0,"600 L/s","700 L/s","ambient","ambient","ambient",0,700,900,"TP-503B"]
[17,"Compressed Air",null,"21050-CSI-PR-PID-009","Gas","Quick Fit","Poly urethane","3/8\"","1.6mm","-","5/60","0/2500","-","-","-","Ambient min","Ambient","Ambient Max",0,600,900,"TP-504"]
["Valley Beater"]
[18,"Main Water Supply",null,"21050-CSI-PR-PID-009","Liquid","To Atmosphere","Copper","15 mm",null,"Class 2","5/40","0/1500",0,"600 L/s","700 L/s","ambient","ambient","ambient",0,700,900,"TP-505"]
[19,"Hot water",null,"21050-CSI-PR-PID-009","Liquid","To Atmosphere","Copper","15 mm",null,"Class 2","5/65","0/1500",0,"190 L/h\n0.05 L/s","*1.9 L/s\nDrainig from the 250 L",28,"50",60,0,300,400,"TP-506"]
["Pilot BioChar Unit"]
[20,"Main Water Supply",null,"21050-CSI-PR-PID-006","Liquid","BSP Thread",304,"1/2\"",null,null,"5/40","0/1500","0 LPH",null,"20 LPH","ambient","ambient","ambient",0,700,900,"TP-401"]
["Gas Line"]
[21,"Compressed Air",null,"21050-CSI-PR-PID-010","Gas"," Compression fittings","Copper","12.7 mm (1/2\")",null,"Medical","5/60","0/2500",0,null,null,30,"50",50,0,1000,1600,"TP-601"]
[22,"Nitrogen",null,"21050-CSI-PR-PID-010","Gas"," Compression fittings","Copper","9.53 mm (3/8\")",null,"Medical","5/40","0/2500",0,"-","-","ambient","ambient","ambient",0,2000,2200,"TP-602"]
["Liquid Line"]
[23,"Municipal Water Supply",null,"21050-CSI-PR-PID-011","Liquid"," Compression fittings","Copper","15/22 mm",null,"Class 2","5/40","0/1500",0,"600 L/s","700 L/s","ambient","ambient","ambient",0,700,900,"TP-801","Various  possible tie in point\nFlow rate is estimated from floe meter reading."]
[24,"Hot water",null,"21050-CSI-PR-PID-011","Liquid"," Compression fittings","Copper","22 mm",null,"Class 2","5/65","0/1500",0,"190 L/h\n0.05 L/s","*1.9 L/s\nDrainig from the 250 L",28,"50",60,0,300,400,"TP-802","\nHeat pump has an estimsated heat capapcity of 70l/h with an 4kW (120L/h) geyser, with a 250 L tank."]
["Boiler"]
[25,"Municipal Water Supply",null,"21050-CSI-PR-PID-012","Liquid","Compression Fitting - Male BSP","Brass-Iron","3/4\"",null,"Class 2","0/40","0/1500",{"$nulls":3},"ambient","ambient","ambient",0,700,"TBC"]
[26,"Main Steam Outlet",null,"21050-CSI-PR-PID-012","Vapour","EN 1092-2500/3 Flange","Carbon Steel","2\"","SCH 40",null,"5/207.17","0/1700",{"$nulls":3},120.24,184.13,207.17,"1 00",1000,1700]
[27,"Safety Valve Outlet",null,"21050-CSI-PR-PID-012","Vapour","BSP Screwed","Mild Steel","1\"","SCH 40",null,"5/207.17","0/1700",{"$nulls":3},0,"N/A",207.17]
[28,"Blowdown Tank Drain",null,"21050-CSI-PR-PID-012","Liquid","BSP Screwed","Mild Steel","1 1/2\"\"","SCH 40",null,"5/207.17","0/1700",{"$nulls":3},120.24,184.13,207.17,"1 00",1000,1700]
[29,"Feed Water Tank Ball Valve",null,"21050-CSI-PR-PID-012","Liquid","Compression Fitting - Male BSP","Copper","3/4\"",null,"Class 2","5/90","0/1500",{"$nulls":3},0,"ambient",40]
[30,"Vent on Feed Tank",null,"21050-CSI-PR-PID-012","Liquid","BSP Screwed","Mild Steel","2\"","SCH 40",null,100,"Open to Atmosphere",{"$nulls":3},"Ambient","Ambient","Ambient"]
[31,"Vent on Blowdown Tank",null,"21050-CSI-PR-PID-012","Vapour","BSP SCrewed","Mild Steel","2\"","SCH 40",null,100,"Open to Atmosphere",{"$nulls":3},"<120.24","<184.13","<207.17"]
["Notes",{"$nulls":11},"References"]
[1,"Durban water supply  by law http://www.durban.gov.za/City_Services/water_sanitation/Bylaws_Tariffs/Bylaws/Pages/Water_Supply_Bylaws.aspx"]
[2,"SANS 460 Plain-ended solid drawn copper tubes for potable water"]
[3,null,"Design condition determine from pipeline design"]
[4,null,"Assumed tie-in properties"]