{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["3D printing room"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"3D printing room","index":0,"n_rows":119,"n_cols":6,"rows_kept":119}
[null,"3D PRINTING ROOM ","UNIT ","QUANTITY","RATE","AMOUNT"]
[null,"BUILDING 17A CSIR "]
[]
[]
[]
[null,"Notes "]
[null,"All quantities are re-measurable,"]
[null,"No work shall exceed the recommended BOQ quantities."]
[null,"Additional works are subject to prior approval of client."]
[]
[null,"All works to be completed as per relevant SANS codes, building regulations and as per manufactures recommendations and procedures"]
[]
[null,"Bidder/ contractor to make himself aware of all related SANS coded in terms works required. Also refer to suitable construction standards and manufacturers recommendations for full specifications and application processes."]
[]
[]
[]
[]
[null,"ALUMINIUM STRUCTURE NOTES'"]
[]
[null,"Final Structure to be as per drawing supplied."]
[]
[null,"Aluminium shopfront panels to have minimum height of 2500mm from finished floor level to underside of ceiling"]
[]
[null,"Aluminium structure to consist of subframe as part of support "]
[null,"including horizontal members to assist and transfer iso panel ceiling weight, to ground."]
[]
[null,"Ceiling and Roof,"]
[null,"Ceiling and roof to be one member constructed of prefabricated ISO panels (closed cell polystyrene panel laminated between outer layer of pre-stressed metal sheeting on both sides)"]
[null,"Fitted to aluminium structure as recommended by manufacturer"]
[]
[null,"Supply and install aluminium Shop-front and doors as per drawing consisting of safety glass with natural anodised aluminium frame. Note Allow for glazing certificate of compliance and installation to be done by approved installer, AAAMSA Association of Architectural Aluminium Manufacturers of South Africa"]
[null,"Note, the new aluminium shopfronts to match design of existing panels (indicated on site)"]
[]
[]
[]
[null,"PRICING"]
[]
[]
[{"v":1,"d":"1 "},"DESIGN OF STRUCTURE"]
[null,"Make allowance for the final detailed structural drawing indicating complete design. Including submission for municipal approval","Item",1,null,{"$f":"D40*E40","v":0}]
[null,"Client to first approve and sign off on detailed shop drawings before commencement of manufacture and installation"]
[]
[]
[]
[]
[]
[]
[{"v":2,"d":"2 "},"ALUMINIUM SUPPORT SUBFRAME"]
[null,"Supply and install aluminium subframe with members (size 160 X 60mm) As support for shop front to be fitted too. Installation to be done by approved installer, AAAMSA Association of Architectural Aluminium Manufacturers of South Africa","Item",1,null,{"$f":"D49*E49","v":0}]
[null,"Estimated members "]
[null,"4300mm long X 4 horizontals in width of structure "]
[null,"5800mm long X 4  horizontals in length of structure"]
[null,"2500mm long X 8 posts "]
[]
[{"v":3,"d":"3 "},"SHOPFRONTS"]
[null,"Note all members of structure to be designed and sizes verified prior to manufacturing."]
[null,"Supply and install aluminium Shop-front as per drawing consisting of safety glass with natural anodised aluminium frame. Note Allow for glazing certificate of compliance and installation to be done by approved installer, AAAMSA Association of Architectural Aluminium Manufacturers of South Africa"]
[null,"In panel sizes"]
[null," (± 5800 x 2 700mm)  EXTERNAL PANEL","No",1,null,{"$f":"D59*E59","v":0}]
[null," (± 4300 x 2 700mm) EXTERNAL PANEL","No",1,null,0]
[null," (± 4250 x 2 700mm) INTERNAL PANEL","No",1,null,0]
[]
[]
[{"v":4,"d":"4 "},"INTERNAL AND ENTRANCE DOORS"]
[null,"Supply and install aluminium single doors as per drawing consisting of safety glass with natural anodised aluminium frame. Note Allow for glazing certificate of compliance and installation to be done by approved installer, AAAMSA Association of Architectural Aluminium Manufacturers of South Africa","no",2,null,{"$f":"D65*E65","v":0}]
[]
[]
[{"v":5,"d":"5 "},"SANDWICH PANELS"]
[null,"Note all members of structure to be designed and sizes verified prior to manufacturing."]
[null,"Supply and install isoboard sandwich panels as per manufactures specification, to be installed as fixed roof over structure"]
[null,"Panels to be 50mm thick closed cell polystyrene panel laminated between outer layer pre-stressed metal sheeting on both sides"]
[null,"Roof."]
[]
[null," (± 5800 x 4300mm)  ROOF PANEL","m2",{"$f":"6*4.5","v":27},null,{"$f":"D74*E74","v":0}]
[]
[null,"Extra panel to close opening between roof/ceiling and existing aluminium partitioning"]
[null,"In panel sizes"]
[null," (± 5800 x 300mm)  SIDE PANEL","m2",6,null,{"$f":"D78*E78","v":0}]
[]
[null,"Aluminium edge trims for roof"]
[null,"Supply and install aluminium edge caping all-round the roof to close off all openings","m",30,null,{"$f":"D81*E81","v":0}]
[null,"Supply and install aluminium support angle caping as part of support base for the iso side panel.","m",{"$f":"6*3","v":18},null,{"$f":"D82*E82","v":0}]
[]
[]
[]
[{"v":6,"d":"6 "},"WINDOW FROSTING"]
[null,"All lower shopfront panels to receive frosting as per existing freestanding frame","m2",20,null,{"$f":"D87*E87","v":0}]
[]
[]
[]
[{"v":7,"d":"7 "},"RUBBLE REMOVAL"]
[null,"Allow for removal of all contractor's rubble ","Item",1,null,{"$f":"D92*E92","v":0}]
[]
[{"v":8,"d":"8 "},"SAFETY FILE"]
[null,"Safety file allowance","Item",1,null,{"$f":"D95*E95","v":0}]
[]
[]
[]
[{"v":9,"d":"9 "},"PROVISIONAL AMOUNTS"]
["9.1.","Mechanical Extraction","Item",1,60000,{"v":60000,"d":"R60,000.00"}]
[]
["9.2.","Electrical","Item",1,40000,{"v":40000,"d":"R40,000.00"}]
{"$rows_empty":7}
[null,null,"Subtotal ",null,null,0]
[]
[]
[null,"Contingency",{"v":0.1,"d":"10%"},null,null,{"$f":"F110*C113","v":0}]
[]
[null,null,"subtotal",null,null,{"$f":"F110+F113","v":0}]
[]
[null,null,"VAT",null,null,{"$f":"F115*0.15","v":0}]
[]
[null,null,"Total Price",null,null,{"$f":"F115+F117","v":0}]