{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Technical Spec","Sheet1"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Technical Spec","index":0,"n_rows":72,"n_cols":9,"rows_kept":72,"merged":[[71,0,71,2]]}
[]
["Typical Application","Fixture\n Type","Existing Lamp \n Type"," Quantity of fixtures","Number of lamps per fixture","Existing lamp rating [W]","Light Output (Lumens)","Proposed \nSolution ","Solution\n Cost"]
["General internal areas","Ball Fixture","CFL",144,1,50,600]
["General internal areas","Ball Fixture","CFL",3,1,11,600]
["General internal areas","Ball Fixture","CFL",4,1,11,600]
["General internal areas","Bulkhead","2D ",2,1,16,600]
["General internal areas","Bulkhead","CFL",35,2,14,600]
["General internal areas","Bulkhead","Incandescent",4,1,100,600]
["General internal areas","Bulkhead","PL9",6,2,9,600]
["General internal areas","Bulkhead","PL-9",2,2,9,600]
["General internal areas","Ceiling Mounted Diffuser","T8L36",2,2,36,3350]
["General internal areas","Ceiling Mounted Diffuser","T8L58",23,2,58,5200]
["General internal areas","Ceiling Mounted Louvre","T8L36",5,3,36,3350]
["General internal areas","Ceiling Mounted Louvre","T8L58",31,2,58,5200]
["General internal areas","Ceiling Recessed","CFL",6,1,14,600]
["General internal areas","Ceilling Recessed","Incandescent",10,1,60,600]
["General internal areas","CFL","Bulbs",11,1,11,600]
["General internal areas","Closed Channel","CFL",1,1,11,600]
["General internal areas","Closed Channel","T5L18",3,3,18,1200]
["General internal areas","Closed Channel","T5L36",1,3,36,3100]
["General internal areas","Closed Channel","T5L75",2,2,75,6150]
["General internal areas","Closed Channel","T8L18",1,3,18,1200]
["General internal areas","Closed Channel","T8L36",229,4,48,3350]
["General internal areas","Closed Channel","T8L38",1,1,38,3100]
["General internal areas","Closed Channel","T8L58",1,2,58,5200]
["General internal areas","closed chgannel","T12L58",2,2,58,5200]
["General internal areas","Downlight","Halogen",52,1,50,600]
["General internal areas","Dustproof","T8L58",2,2,58,5200]
["General internal areas","E27","CFL",59,1,50,600]
["General internal areas","closed chgannel","T8L36",1,2,36,3350]
["General internal areas","Flameproof","T8L36",2,2,36,3350]
["General internal areas","Flameproof","T8L58",4,2,58,5200]
["General Workshop/Warehouse Areas","Flood","HPS",6,1,250,36000]
["General Workshop/Warehouse Areas","Flood","Mercury Vapor",30,1,400,36000]
["General Workshop/Warehouse Areas","Flood Light","Mercury Vapor",3,1,400,36000]
["General Workshop/Warehouse Areas","Flood Lights","Mercry Vapor",14,1,400,36000]
["General Workshop/Warehouse Areas","Low Bay","Mercury Vapor",10,3,400,36000]
["General external areas","Metal Halide","Post Top, MH , HID 70W",11,1,70,36000]
["General Workshop/Warehouse Areas","Metal Halide","Round Street Light, MH , HID 400W",54,1,400,36000]
["General internal areas","Mounted Diffuser","T8L58",6,2,58,5200]
["General Workshop/Warehouse Areas","Low Bay","Mercury Vapor",34,1,400,36000]
["General internal areas","Open Channel","Bulbs",19,8,50,600]
["General internal areas","Open Channel","CFL",26,1,11,600]
["General internal areas","Open Channel","T12L40",13,2,40,3100]
["General internal areas","Open Channel","T12L65",27,2,65,5200]
["General internal areas","Open Channel","T12L75",199,2,75,6150]
["General internal areas","Open Channel","T5L18",4,3,18,1200]
["General internal areas","Open Channel","T5L36",1,2,36,3100]
["General internal areas","Open Channel","T5L53",2,2,53,5200]
["General internal areas","Open Channel","T5L54",51,2,54,5200]
["General internal areas","Open Channel","T5L65",1,2,65,5200]
["General internal areas","Open Channel","T5L75",14,2,75,6150]
["General internal areas","Open Channel","T5L78",4,2,36,3100]
["General internal areas","Open Channel","T5L79",4,2,58,5200]
["General internal areas","Open Channel","T8L18",9,3,18,1200]
["General internal areas","Open Channel","T8L36",435,4,58,3350]
["General internal areas","Open Channel","T8L40",30,2,40,3100]
["General internal areas","Open Channel","T8L58",1004,4,58,5200]
["General internal areas","Open Channel","T8L65",10,2,65,5200]
["General internal areas","Open Channel","T8L75",5,2,75,6150]
["General internal areas","Open Channel","T8LED",3,2,24,600]
["General internal areas","Pendant","CFL",2,3,14,600]
["General internal areas","Recessed","CFL",2,1,11,600]
["General internal areas","Recessed","Halogen",3,1,20,600]
["General internal areas","Recessed Diffuser","T8L18",63,4,18,1200]
["General internal areas","Recessed Diffuser","T8L36",512,3,36,3350]
["General internal areas","Recessed Louvre","T5L28",19,3,28,3100]
["General internal areas","Recessed Louvre","T5L54",5,3,54,5200]
["General internal areas","Recessed Louvre","T8L36",18,3,36,3350]
["General internal areas","Vaporproof","T5L54",2,2,54,5200]
["General internal areas","Vaporproof","T8L65",4,2,65,5200]
["Total ",null,null,{"$f":"SUM(D3:D71)","v":3308}]

{"sheet":"Sheet1","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}