{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["BP - BOQ","SMF - BOQ","5.7 Sum"],"not_rendered":{"images":2,"external_links":22,"defined_names":1213},"read":"whole","date_system":"1900"}

{"sheet":"BP - BOQ","index":0,"n_rows":223,"n_cols":8,"rows_kept":223}
[]
[]
["C4021 - CSIR 3457 PHARMA - WET SERVICES - PRICE BREAKDOWN SCHEDULE - BP"]
[]
["SCHEDULE NO.1 : BP FOUL SEWER DRAINAGE SYSTEM"]
["(Note : These prices shall be firm and not subject to price adjustment)"]
["Item","Description","Unit","QTY","Supply Rate","Total Supply","Install Rate","Amount"]
[null,"Work shall comply with the relevant conditions and installation specifications of SANS 10252-2, manufacturers specifications and local By-laws and Regulations. Contractor shall issue a certificate of compliance in terms of local By-laws upon completion. All works, equipment and practices shall be SABS complient and equipment stamped as such.\n"]
[null,"Rates shall include allowance for fixings and bracketing of piping reticulation to walls and soffits."]
[]
[null,"FOUL SEWER DRAINAGE"]
[]
[1.1,"Supply and install Geberit HDPE, or equal alternative pipe:"]
[]
[1,"40mm pipe","m",4.5]
[2,"56mm pipe","m",0]
[3,"63mm pipe","m",31]
[4,"75mm pipe","m",0]
[5,"110mm pipe","m",29]
[]
[6,"50mm-50mm-50mm 45° branch junction","no",0]
[7,"56mm-56mm-56mm 45° branch junction","no",0]
[8,"63mm-63mm-40mm 45° branch junction","no",4]
[9,"63mm-63mm-56mm 45° branch junction","no",1]
[10,"63mm-63mm-63mm 45° branch junction","no",3]
[11,"75mm-75mm-63mm 45° branch junction","no",0]
[12,"110mm-110mm-63mm 45° branch junction","no",4]
[12,"110mm-110mm-110mm 45° branch junction","no",1]
[null,""]
[13,"63mm-63mm-63mm-63mm 45° double branch junction","no",1]
[]
[14,"40mm 45° bend","no",13]
[15,"50mm 45° bend","no",0]
[16,"63mm 45° bend","no",23]
[17,"110mm 45° bend","no",2]
[]
[18,"40 x 32mm reducer","no",12]
[19,"50 x 40mm reducer","no",1]
[20,"63 x 40mm reducer","no",8]
[21,"110 x 75mm reducer","no",0]
[22,"110 x 63mm reducer","no",1]
[]
[23,"56mm rodding eye and cap","no",0]
[24,"63mm rodding eye and cap","no",5]
[25,"110mm rodding eye and cap","no",0]
[]
[26,"75mm screw on stopend & one way vent valve (air admittance valve)","no",2]
[27,"63mm HDPE Anti-siphon Bottle Trap","no",9]
[28,"Supply and install new gulley","no",0]
[29,"Connect to existing sewer piping","no",3]
[]
[1.2,"Test drainage installation.","sum",1]
[]
[]
[]
["Total for Schedule No. 1 Carried forward to summary page",{"$nulls":5},"R"]
[]
[]
["SCHEDULE NO. 2 : BP COLD WATER PIPING "]
["(Note : These prices shall be firm and not subject to price adjustment)"]
["Item","Description","Unit",null,"Supply Rate","Total Supply","Install Rate","Amount"]
[null,"Work shall comply with the relevant conditions and installation specifications of SANS 10252-1, manufacturers specifications and local By-laws and Regulations. Sub-Contractor shall issue a certificate of compliance in terms of local By-laws upon completion. All works, equipment and practices shall be SABS compliant and equipment stamped as such.\n"]
[null,"Rates shall include allowance for fixings and bracketing of piping reticulation to walls and soffits."]
[]
[null,"COLD WATER SUPPLY"]
[]
[2.1,"Supply and install Copper class 2, or equal alternative, pipe (outside diameter):"]
[]
[1,"15mm pipes","m",94]
[2,"22mm pipes","m",12]
[3,"28mm pipes","m",12]
[]
[2.2,"Supply and install DZR Brass fittings:"]
[]
[1,"15mm 90º bend","no",51]
[2,"22mm 90º bend","no",5]
[3,"28mm 90º bend","no",5]
[]
[4,"22 mm x 15 mm reducer","no",9]
[5,"28 mm x 15 mm reducer","no",4]
[6,"28 mm x 22 mm reducer","no",1]
[6,"35 mm x 15 mm reducer","no",1]
[]
[7,"15 x 15 x 15mm tee junction","no",3]
[8,"22 x 22 x 22mm tee junction","no",7]
[9,"28 x 28 x 28mm tee junction","no",4]
[]
[2.3,"Supply and install valves including threaded capillary fittings for connection to sanitary fixtures, etc. to copper pipe:"]
[]
[1,"15mm stop valve","no",12]
[2,"22mm stop valve","no",0]
[3,"Air relieve valve","no",0]
[4,"Termostatic Mixing Valve","no",0]
[]
[4,"25mm Pressure reducing valve with guage","no",1]
[5,"22mm Non-return valve","no",1]
[]
[2.4,"Connect to existing water supply pipe","sum",1]
[]
[2.5,"Testing of complete installed cold water system.","sum",1]
[]
[]
["Total for Schedule No. 2 Carried forward to summary page",{"$nulls":5},"R"]
[]
[]
["SCHEDULE NO.3 : BP HOT WATER PIPING"]
["(Note : These prices shall be firm and not subject to price adjustment)"]
["Item","Description","Unit",null,"Supply Rate","Total Supply","Install Rate","Amount"]
[null,"Work shall comply with the relevant conditions and installation specifications of SANS 10252-1, manufacturers specifications and local By-laws and Regulations. Sub-Contractor shall issue a certificate of compliance in terms of local By-laws upon completion. All works, equipment and practices shall be SABS compliant and equipment stamped as such.\n"]
[null,"Rates shall include allowance for fixings and bracketing of piping reticulation to walls and soffits."]
[]
[null,"HOT WATER SUPPLY AND RETURN"]
[]
[3.1,"Supply and install insulated Copper class 2, or equal alternative, pipe (outside diameter):"]
[]
[1,"15mm pipes","m",63]
[2,"22mm pipes","m",10]
[2,"28mm pipes","m",19]
[]
[3.2,"Supply and install insulated DZR Brass fittings:"]
[]
[1,"15mm 90º bend","no",47]
[2,"22mm 90º bend","no",15]
[]
[3,"22 mm x 15 mm reducer","no",5]
[4,"28 mm x 15 mm reducer","no",3]
[]
[5,"15 x 15 x 15mm tee junction","no",6]
[6,"22 x 22 x 22mm tee junction","no",4]
[6,"28 x 28 x 28mm tee junction","no",0]
[]
[3.3,"Supply and install valves including threaded capillary fittings for connection to sanitary fixtures, etc. to copper pipe:"]
[]
[1,"15mm stop valve","no",8]
[2,"15mm Non-return valve","no",1]
[3,"Air relieve valve","no",2]
[4,"15mm Strainer","no",1]
[4,"Globe Valve","no",3]
[]
[3.4,"Testing of complete installed hot water system.","sum",1]
[]
["Total for Schedule No. 3 Carried forward to summary page",{"$nulls":5},"R"]
[]
[]
["SCHEDULE NO. 4 : BP HOT WATER GENERATION PLANT "]
["Item","Description","Unit","QTY","Supply Rate",null,"Install Rate","Amount"]
[null,"Work shall comply with the relevant conditions and installation specifications of SANS 10252-1, SANS 10254, manufacturers specifications and local By-laws and Regulations. Sub-Contractor shall issue a certificate of compliance in terms of local By-laws upon completion. All works, equipment and practices shall be SABS compliant and equipment stamped as such."]
[]
[4.1,"Hot water generation plant: Procurement, supply, manufacture, delivery to site, storage and installation of:"]
[]
[1,"Heat Pump: KWIKOT c/w a circulating water pump, electronic expansion valve, four-way valve and all associated fittings and consumables required for a fully complete, working system as per layouts..","no",1]
[2,"Hot Water Geyser: KWIKOT DUAL SUPERLINE 150 litre c/w 3kW backup elements, electrical connecton, drip tray and electric water heater blanket and all associated fittings and consumables required for a fully complete, working system.","no",1]
[3,"Circulation Pump: 0,009 kW Lowara ecocirc PRO 15-1/110 U or Equal ","no",1]
[4,"All copper class 2 pipework and fittings - insulation, valves, y-strainers, pump fittings, pressure gauges etc. as per the concept design drawings for a complete and fully functioning hot water installation.","sum",1]
[5,"Bluechem corrosion protection for heat pump","no",1]
[6,"Instantanious Water Boiler with connection and fittings","no",1]
[]
[4.2,"All other equipment, not listed, required for a fully working complete system.","sum",1]
[]
["Total for Schedule No. 4 carried forward to summary page",{"$nulls":5},"R"]
[]
[]
["SCHEDULE NO. 5 : BP GENERAL ITEMS"]
["Item","Description","Unit","QTY","Supply Rate",null,"Install Rate","Amount"]
[]
[]
[1,"Complete set of operation manuals and as-built drawings","sum",1]
[]
[2,"Install and connect the emergency shower (supplied by others)","sum",0]
[]
[3,"Connection of water supply to the following fittings:"]
[3.1,"Laboratory double sink","sum",0]
[3.2,"Laboratory single sink","sum",1]
[3.3,"Wash hand basin","sum",2]
[3.4,"Eye showers","sum",2]
[]
[4,"Connection of bottle traps and drainage to the following fittings:"]
[4.1,"Laboratory double sink","sum"]
[4.2,"Laboratory single sink","sum",1]
[4.3,"Wash hand basin","sum",2]
[]
[5,"12 month maintenance","sum",1]
[]
["Total for Schedule No. 5 carried forward to summary page",{"$nulls":5},"R"]
[]
[]
["SUMMARY OF BILLS OF QUANTITIES"]
[]
["Item","Description",{"$nulls":5},"Sub-Total"]
[]
[1,"TOTAL FOR SCHEDULE NO. 1"]
[2,"TOTAL FOR SCHEDULE NO. 2"]
[3,"TOTAL FOR SCHEDULE NO. 3"]
[4,"TOTAL FOR SCHEDULE NO. 4"]
[5,"TOTAL FOR SCHEDULE NO. 5"]
[]
[]
[]
[]
[]
[null,"TOTAL FOR BILLS OF QUANTITIES (excl. VAT)",{"$nulls":4},"R"]
[]
[]
["Item","Description","Unit","Rate","Amount",null,null,"Sub-Total"]
[null,"PLUMBING AND DRAINAGE  INSTALLATION"]
[]
["A","Price Breakdown Schedules No. 1 TO 5"]
[null,"Subtotal"]
[]
[]
[null,"Provisional Amounts for :"]
["B"]
["C"]
["D"]
["E"]
[null,"Subtotal for B+C+D+E"]
[]
[null,"TOTAL NET CONTRACT SUM (excl vat)"]
[{"$nulls":6},"R"]
[1,"Above Total Net contract sum to be carried forward to Principal Contract Form of Tender"]
[null,"contained in this document."]
[2,"All the rates in this document must be supplied."]
[3,"Above amounts to exclude VAT."]

{"sheet":"SMF - BOQ","index":1,"n_rows":208,"n_cols":8,"rows_kept":208}
[]
[]
["C4021 - CSIR 3457 PHARMA - WET SERVICES - PRICE BREAKDOWN SCHEDULE - SMF"]
[]
["SCHEDULE NO.1 : SMF FOUL SEWER DRAINAGE SYSTEM"]
["(Note : These prices shall be firm and not subject to price adjustment)"]
["Item","Description","Unit","QTY","Supply Rate","Total Supply","Install Rate","Amount"]
[null,"Work shall comply with the relevant conditions and installation specifications of SANS 10252-2, manufacturers specifications and local By-laws and Regulations. Contractor shall issue a certificate of compliance in terms of local By-laws upon completion. All works, equipment and practices shall be SABS complient and equipment stamped as such.\n"]
[null,"Rates shall include allowance for fixings and bracketing of piping reticulation to walls and soffits."]
[]
[null,"FOUL SEWER DRAINAGE"]
[]
[1.1,"Supply and install Geberit HDPE, or equal alternative pipe:"]
[]
[1,"40mm pipe","m",7.5]
[2,"56mm pipe","m",0]
[3,"63mm pipe","m",40]
[4,"75mm pipe","m"]
[5,"110mm pipe","m",67]
[]
[6,"50mm-50mm-50mm 45° branch junction","no",0]
[7,"56mm-56mm-56mm 45° branch junction","no",0]
[8,"63mm-63mm-40mm 45° branch junction","no",10]
[9,"63mm-63mm-56mm 45° branch junction","no",0]
[10,"63mm-63mm-63mm 45° branch junction","no",6]
[11,"75mm-75mm-63mm 45° branch junction","no",0]
[12,"110mm-110mm-63mm 45° branch junction","no",4]
[13,"110mm-110mm-110mm 45° branch junction","no",7]
[null,""]
[14,"63mm-63mm-63mm-63mm 45° double branch junction","no",0]
[]
[15,"40mm 45° bend","no",12]
[16,"50mm 45° bend","no"]
[17,"63mm 45° bend","no",50]
[18,"110mm 45° bend","no",16]
[]
[19,"40 x 32mm reducer","no",14]
[20,"63 x 40mm reducer","no",10]
[21,"75 x 63mm reducer","no",{"v":0,"d":"0.000"}]
[22,"110 x 63mm reducer","no",0]
[]
[23,"56mm rodding eye and cap","no",0]
[24,"63mm rodding eye and cap","no",7]
[25,"75mm rodding eye and cap","no",0]
[]
[26,"75mm screw on stopend & one way vent valve (air admittance valve)","no",0]
[27,"63mm HDPE Anti-siphon Bottle Trap","no",19]
[28,"Supply and install 1000L sludge tank complete with level switch required in grease trap in order to activate pump, include all required valves for pump installation.","no",1]
[29,"Connect to existing sewer piping","no",3]
[]
[1.2,"Test drainage installation.","sum",1]
[]
[]
[]
["Total for Schedule No. 1 Carried forward to summary page",{"$nulls":5},"R"]
[]
[]
["SCHEDULE NO.2 : SMF COLD WATER PIPING "]
["(Note : These prices shall be firm and not subject to price adjustment)"]
["Item","Description","Unit",null,"Supply Rate","Total Supply","Install Rate","Amount"]
[null,"Work shall comply with the relevant conditions and installation specifications of SANS 10252-1, manufacturers specifications and local By-laws and Regulations. Sub-Contractor shall issue a certificate of compliance in terms of local By-laws upon completion. All works, equipment and practices shall be SABS compliant and equipment stamped as such.\n"]
[null,"Rates shall include allowance for fixings and bracketing of piping reticulation to walls and soffits."]
[]
[null,"COLD WATER SUPPLY"]
[]
[2.1,"Supply and install Copper class 2, or equal alternative, pipe (outside diameter):"]
[]
[1,"15mm pipes","m",60]
[2,"22mm pipes","m",45]
[3,"28mm pipes","m",4]
[4,"35mm pipes","m",19]
[]
[2.2,"Supply and install DZR Brass fittings:"]
[]
[1,"15mm 90º bend","no",58]
[2,"22mm 90º bend","no",26]
[]
[3,"22 mm x 15 mm reducer","no",25]
[4,"28 mm x 22 mm reducer","no",3]
[5,"35 mm x 15 mm reducer","no",3]
[6,"35 mm x 22 mm reducer","no",4]
[7,"35 mm x 28 mm reducer","no",1]
[]
[8,"15 x 15 x 15mm tee junction","no",9]
[9,"22 x 22 x 22mm tee junction","no",13]
[10,"28 x 28 x 28mm tee junction","no",1]
[11,"35 x 35 x 35mm tee junction","no",5]
[]
[2.3,"Supply and install valves including threaded capillary fittings for connection to sanitary fixtures, etc. to copper pipe:"]
[]
[1,"15mm stop valve","no",17]
[2,"22mm stop valve","no",8]
[3,"Air relieve valve","no",0]
[4,"Termostatic Mixing Valve","no",2]
[]
[4,"25mm Pressure reducing valve with guage","no",0]
[5,"35mm Non-return valve","no",1]
[]
[2.4,"Connect to existing water supply pipe","sum",1]
[]
[2.5,"Testing of complete installed cold water system.","sum",1]
[]
[]
["Total for Schedule No. 2 Carried forward to summary page",{"$nulls":5},"R"]
[]
[]
["SCHEDULE NO.3 : SMF HOT WATER PIPING"]
["(Note : These prices shall be firm and not subject to price adjustment)"]
["Item","Description","Unit",null,"Supply Rate","Total Supply","Install Rate","Amount"]
[null,"Work shall comply with the relevant conditions and installation specifications of SANS 10252-1, manufacturers specifications and local By-laws and Regulations. Sub-Contractor shall issue a certificate of compliance in terms of local By-laws upon completion. All works, equipment and practices shall be SABS compliant and equipment stamped as such.\n"]
[null,"Rates shall include allowance for fixings and bracketing of piping reticulation to walls and soffits."]
[]
[null,"HOT WATER SUPPLY AND RETURN"]
[]
[3.1,"Supply and install insulated Copper class 2, or equal alternative, pipe (outside diameter):"]
[]
[1,"15mm pipes","m",131]
[2,"22mm pipes","m",15]
[3,"28mm pipes","m",0]
[]
[3.2,"Supply and install insulated DZR Brass fittings:"]
[]
[1,"15mm 90º bend","no",25]
[2,"22mm 90º bend","no",5]
[]
[3,"22 mm x 15 mm reducer","no",3]
[4,"28 mm x 15 mm reducer","no",4]
[4,"28 mm x 22 mm reducer","no",4]
[]
[6,"15 x 15 x 15mm tee junction","no",2]
[7,"22 x 22 x 22mm tee junction","no",3]
[8,"28 x 28 x 28mm tee junction","no",5]
[]
[3.3,"Supply and install valves including threaded capillary fittings for connection to sanitary fixtures, etc. to copper pipe:"]
[]
[1,"15mm stop valve ","no",6]
[2,"22mm stop valve","no",3]
[2,"15mm Non-return valve","no",0]
[3,"Air relieve valve","no",0]
[4,"15mm Strainer","no",0]
[5,"Globe Valve","no",1]
[]
[3.4,"Testing of complete installed hot water system.","sum",1]
[]
["Total for Schedule No. 3 Carried forward to summary page",{"$nulls":5},"R"]
[]
[]
["SCHEDULE NO. 4 : SMF GENERAL ITEMS"]
["Item","Description","Unit","QTY","Supply Rate",null,"Install Rate","Amount"]
[]
[]
[1,"Complete set of operation manuals and as-built drawings","sum",1]
[]
[2,"Install and connect the emergency shower (supplied by others)","sum",2]
[]
[3,"Connection of water supply to the following fittings:"]
[3.1,"Laboratory double sink","sum",2]
[3.2,"Laboratory single sink","sum",0]
[3.3,"Wash hand basin","sum",4]
[3.4,"Eye showers","sum",3]
[]
[4,"Connection of bottle traps and drainage to the following fittings:"]
[4.1,"Laboratory double sink","sum",2]
[4.2,"Laboratory single sink","sum",4]
[4.3,"Wash hand basin","sum"]
[]
[5,"12 month maintenance","sum",1]
[]
["Total for Schedule No. 4 carried forward to summary page",{"$nulls":5},"R"]
[]
[]
["SUMMARY OF BILLS OF QUANTITIES"]
[]
["Item","Description",{"$nulls":5},"Sub-Total"]
[]
[1,"TOTAL FOR SCHEDULE NO. 1"]
[2,"TOTAL FOR SCHEDULE NO. 2"]
[3,"TOTAL FOR SCHEDULE NO. 3"]
[4,"TOTAL FOR SCHEDULE NO. 4"]
[]
[]
[]
[]
[]
[]
[null,"TOTAL FOR BILLS OF QUANTITIES (excl. VAT)",{"$nulls":4},"R"]
[]
[]
["Item","Description","Unit","Rate","Amount",null,null,"Sub-Total"]
[null,"PLUMBING AND DRAINAGE  INSTALLATION"]
[]
["A","Price Breakdown Schedules No. 1 TO 4"]
[null,"Subtotal"]
[]
[]
[null,"Provisional Amounts for :"]
["B"]
["C"]
["D"]
["E"]
[null,"Subtotal for B+C+D+E"]
[]
[null,"TOTAL NET CONTRACT SUM (excl vat)"]
[{"$nulls":6},"R"]
[1,"Above Total Net contract sum to be carried forward to Principal Contract Form of Tender"]
[null,"contained in this document."]
[2,"All the rates in this document must be supplied."]
[3,"Above amounts to exclude VAT."]

{"sheet":"5.7 Sum","index":2,"n_rows":82,"n_cols":7,"rows_kept":82,"merged":[[53,5,55,5]]}
[]
[]
[]
[]
[null,null,"Wet Services Bills of Quantities"]
[]
["Bill     No",{"$nulls":4},"Amount"]
[]
[5.7,null,"Wet Services Bills of Quantities",null,"R"]
[]
[]
[null,null,"Main Contractors percentage for all mark-ups, attendance, etc on specialist domestic contractor",null,"R"]
{"$rows_empty":41}
[{"$nulls":5},{"$f":"SUM(F9:F13)","v":0}]
[null,null,"Carried Forward To Section 5.10 : Final Summary",null,"R"]
[]
[]
[]
[null,null,"CSIR Future PHARMA Facility"]
[]
[]
[{"$nulls":6},"Section 5.7 : Wet Services Bills of Quantities"]
[{"$nulls":6},"Page No. 11 of 11"]
{"$rows_empty":18}
[null,"References"]