{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Appendix A ","Appendix B","Sheet1"],"not_rendered":{"comments":1},"read":"whole","date_system":"1900"}

{"sheet":"Appendix A ","index":0,"n_rows":37,"n_cols":4,"rows_kept":37,"merged":[[1,1,2,1],[1,2,1,3],[2,2,2,3],[11,1,11,3],[28,1,28,3],[30,2,31,2],[30,3,31,3]]}
[null,"CSIR RFP No: 3179/02/03/2018 - APPENDIX B"]
[null,"Monthly Preventative Maintenance Schedule","Tick the correct space"]
[null,null,"Yes/No"]
[null,"Emerson Maintenance","Yes","No"]
[null,"4.1.1        Check and replace air filters as required."]
[null,"4.1.2        Inspect and clean impellers of debris, check belt tensions and adjust. Verify fan safety switch operation."]
[null,"4.1.3        Check of the infrared humidifier pans for mineral deposits, ensure water make-up valves are not leaking and drains are free of debris."]
[null,"4.1.4        Inspect refrigerant lines and check for proper refrigerant levels, checking for moisture, measuring suction and discharge pressures."]
[null,"4.1.5        Check fuses, tighten connections and verify proper operation sequences as well as contactors for pitting."]
[null,"4.1.6        Thorough cleaning of the air-cooled condenser coil, tightening of the motor mounts, inspects motor bearing and refrigerant lines."]
[null,"4.1.7        Examine the glycol pump for any leaks and determine if it is working properly."]
[null,"Additional checks"]
[null,"4.1.8        Check all motors, electrical circuits, controls"]
[null,"4.1.9        Check coil condition, condenser vibration and function"]
[null,"4.1.10     Check ALL pressures"]
[null,"4.1.11     Check heat rejection off condenser"]
[null,"4.1.12     Check unit overall functionality with regards to configurations, auto-restarts etc"]
[null,"4.1.13     Check environment with regards to temperature, relative humidity"]
[null,"4.1.14     Check unit communication, remote unit response etc"]
[null,"4.1.15     Check overall system for any leaks of any kind"]
[null,"UniFlair Preventative Maintenance","Yes","No"]
[null,"4.2.1 Check and replace air filters as required."]
[null,"4.2.2 Inspect and clean impellers of debris, check belt tensions and adjust. Verify fan safety switch operation."]
[null,"4.2.3 Check of the infrared humidifier pans for mineral deposits, ensure water make-up valves are not leaking and drains are free of debris."]
[null,"4.2.4 Inspect refrigerant lines and check for proper refrigerant levels, checking for moisture, measuring suction and discharge pressures."]
[null,"4.2.5 Check fuses, tighten connections and verify proper operation sequences as well as contactors for pitting."]
[null,"4.2.6 Thorough cleaning of the air-cooled condenser coil, tightening of the motor mounts, inspect motor bearing and refrigerant lines."]
[null,"4.2.7 Examine the glycol pump for any leaks and determine if it is working properly."]
[null," Additional checks"]
[null,"4.2.8 Check all motors, electrical circuits, controls"]
[null,"4.2.9 Check coil condition, condenser vibration and function"]
[null,"4.2.10 Check ALL pressures"]
[null,"4.2.11 Check heat rejection off condenser"]
[null,"4.2.12 Check unit overall functionality with regards to configurations, auto-restarts etc"]
[null,"4.2.13 Check environment with regards to temperature, relative humidity"]
[null,"4.2.14 Check unit communication, remote unit response etc"]
[null,"4.2.15 Check overall system for any leaks of any kind"]

{"sheet":"Appendix B","index":1,"n_rows":112,"n_cols":9,"rows_kept":112,"merged":[[2,1,2,8],[3,1,5,1],[3,2,5,2],[3,3,5,3],[3,8,4,8],[26,1,26,8],[38,1,38,8],[39,1,41,1],[39,2,41,2],[39,3,41,3],[39,8,40,8],[62,1,62,8],[74,1,74,8],[75,1,77,1],[75,2,77,2],[75,3,77,3],[75,8,76,8],[98,1,98,8],[109,3,112,3],[109,8,110,8],[110,1,110,2],[111,1,112,2]]}
[null,"CSIR RFP No: 3179/02/03/2018 - APPENDIX B"]
[null,"Year 1"]
[null,"Ad-hoc Catalogue Pricing, VAT Inclusive"]
[null,"Qty & unit","Part Description","Lead Time","Emerson Liebert","Emerson Liebert","Emerson Liebert","UniFlair","Non-Model Specific"]
[{"$nulls":4},"Model: l83WA001VB","Model: CR035RA","Model: CR020RA","Model: SDA0601A"]
[{"$nulls":4},"Price per Item","Price per Item","Price per Item","Price per Item","Price per Item"]
[null,1,"Expansion Valve","ex-stock"]
[null,1,"Fanspeed Controller","ex-stock"]
[null,1,"HP Switch","ex-stock"]
[null,1,"Teflon Seal","ex-stock"]
[null,1,"Condensor Fan motor","ex-stock"]
[null,1,"Rotor lock seal","ex-stock"]
[null,1,"Humidifier","ex-stock"]
[null,1,"Compressor","ex-stock"]
[null,1,"Humidifier control board","ex-stock"]
[null,1,"Humidifier bottle","ex-stock"]
[null,1,"Humidifier Cylinder","ex-stock"]
[null,1,"Pressure Transducer","ex-stock"]
[null,1,"Recovery Cylinder","ex-stock"]
[null,"11.3 kg",{"v":410,"d":"R 410"},"ex-stock"]
[null,"11.3 kg","R407-C","ex-stock"]
[null,"9 kg","Nitrogen","ex-stock"]
[null,"11.3 kg",{"v":22,"d":"R 22"},"ex-stock"]
[null,"11.3 kg","R141B","ex-stock"]
[null,null,"Total"]
[]
[null,"Adhoc Service rate and time frames"]
[null,null,"Procedures / Services","Duration","Rate per hour"]
[null,null,"Leak Testing duration in man hours"]
[null,null,"System Vacuum and Hold duration in man hours"]
[null,null,"System refrigerent flush duration in man hours"]
[null,null,"Labour after hours"]
[null,null,"Labour Holidays"]
[null,null,"Callout fees"]
[null,null,"Travel fees"]
[]
[]
[null,"Year 2"]
[null,"Ad-hoc Catalogue Pricing, VAT Inclusive"]
[null,"Qty & unit","Part Description","Lead Time","Emerson Liebert","Emerson Liebert","Emerson Liebert","UniFlair","Non-Model Specific"]
[{"$nulls":4},"Model: l83WA001VB","Model: CR035RA","Model: CR020RA","Model: SDA0601A"]
[{"$nulls":4},"Price per Item","Price per Item","Price per Item","Price per Item","Price per Item"]
[null,1,"Expansion Valve","ex-stock"]
[null,1,"Fanspeed Controller","ex-stock"]
[null,1,"HP Switch","ex-stock"]
[null,1,"Teflon Seal","ex-stock"]
[null,1,"Condensor Fan motor","ex-stock"]
[null,1,"Rotor lock seal","ex-stock"]
[null,1,"Humidifier","ex-stock"]
[null,1,"Compressor","ex-stock"]
[null,1,"Humidifier control board","ex-stock"]
[null,1,"Humidifier bottle","ex-stock"]
[null,1,"Humidifier Cylinder","ex-stock"]
[null,1,"Pressure Transducer","ex-stock"]
[null,1,"Recovery Cylinder","ex-stock"]
[null,"11.3 kg",{"v":410,"d":"R 410"},"ex-stock"]
[null,"11.3 kg","R407-C","ex-stock"]
[null,"9 kg","Nitrogen","ex-stock"]
[null,"11.3 kg",{"v":22,"d":"R 22"},"ex-stock"]
[null,"11.3 kg","R141B","ex-stock"]
[null,null,"Total"]
[]
[null,"Adhoc Service rate and time frames"]
[null,null,"Procedures / Services","Duration","Rate per hour"]
[null,null,"Leak Testing duration in man hours"]
[null,null,"System Vacuum and Hold duration in man hours"]
[null,null,"System refrigerent flush duration in man hours"]
[null,null,"Labour after hours"]
[null,null,"Labour Holidays"]
[null,null,"Callout fees"]
[null,null,"Travel fees"]
[]
[]
[null,"Year 3"]
[null,"Ad-hoc Catalogue Pricing, VAT Inclusive"]
[null,"Qty & unit","Part Description","Lead Time","Emerson Liebert","Emerson Liebert","Emerson Liebert","UniFlair","Non-Model Specific"]
[{"$nulls":4},"Model: l83WA001VB","Model: CR035RA","Model: CR020RA","Model: SDA0601A"]
[{"$nulls":4},"Price per Item","Price per Item","Price per Item","Price per Item","Price per Item"]
[null,1,"Expansion Valve","ex-stock"]
[null,1,"Fanspeed Controller","ex-stock"]
[null,1,"HP Switch","ex-stock"]
[null,1,"Teflon Seal","ex-stock"]
[null,1,"Condensor Fan motor","ex-stock"]
[null,1,"Rotor lock seal","ex-stock"]
[null,1,"Humidifier","ex-stock"]
[null,1,"Compressor","ex-stock"]
[null,1,"Humidifier control board","ex-stock"]
[null,1,"Humidifier bottle","ex-stock"]
[null,1,"Humidifier Cylinder","ex-stock"]
[null,1,"Pressure Transducer","ex-stock"]
[null,1,"Recovery Cylinder","ex-stock"]
[null,"11.3 kg",{"v":410,"d":"R 410"},"ex-stock"]
[null,"11.3 kg","R407-C","ex-stock"]
[null,"9 kg","Nitrogen","ex-stock"]
[null,"11.3 kg",{"v":22,"d":"R 22"},"ex-stock"]
[null,"11.3 kg","R141B","ex-stock"]
[null,null,"Total"]
[]
[null,"Adhoc Service rate and time frames"]
[null,null,"Procedures / Services","Duration","Rate per hour"]
[null,null,"Leak Testing duration in man hours"]
[null,null,"System Vacuum and Hold duration in man hours"]
[null,null,"System refrigerent flush duration in man hours"]
[null,null,"Labour after hours"]
[null,null,"Labour Holidays"]
[null,null,"Callout fees"]
[null,null,"Travel fees"]
[]
[]
[{"$nulls":4},"Emerson Liebert","Emerson Liebert","Emerson Liebert","UniFlair","Non-Model Specific"]
[null,"GRAND TOTAL (VAT Inc.)",null,null,"Model: l83WA001VB","Model: CR035RA","Model: CR020RA","Model: SDA0601A"]
[null,"Year 1-3",null,null,"Price per Item","Price per Item","Price per Item","Price per Item","Price per Item"]

{"sheet":"Sheet1","index":2,"n_rows":10,"n_cols":6,"rows_kept":10,"hidden":true}
[null,"Budget","Duration","Brief",null,"Overall customer satisfaction"]
["+/-5%","Within +/- 5% of project budget","Within +/- 5% of total agreed project duration","Yes","Sat","Satisfied"]
["<+10%","Less than 10% over project budget","Less than 10% over agreed project duration","No","S Sat","Somewhat satisfied"]
["<+15%","Less than 15% over project budget","Less than 15% over agreed project duration",null,"S Dissat","Somewhat dissatisfied"]
[">+15%","More than 15% over project budget","More than 15% over agreed project duration",null,"Dissat","Dissatisfied"]
[]
[null,{"$f":"CONCATENATE($A$2,\" - \", B2)","v":"+/-5% - Within +/- 5% of project budget"},{"$f":"CONCATENATE($A$2,\" - \", C2)","v":"+/-5% - Within +/- 5% of total agreed project duration"}]
[null,{"$f":"CONCATENATE($A$3,\" - \", B3)","v":"<+10% - Less than 10% over project budget"},{"$f":"CONCATENATE($A$3,\" - \", C3)","v":"<+10% - Less than 10% over agreed project duration"}]
[null,{"$f":"CONCATENATE($A$4,\" - \", B4)","v":"<+15% - Less than 15% over project budget"},{"$f":"CONCATENATE($A$4,\" - \", C4)","v":"<+15% - Less than 15% over agreed project duration"}]
[null,{"$f":"CONCATENATE($A$5,\" - \", B5)","v":">+15% - More than 15% over project budget"},{"$f":"CONCATENATE($A$5,\" - \", C5)","v":">+15% - More than 15% over agreed project duration"}]