{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["TG-801A","TG-801B","TG-802"],"not_rendered":{"images":2,"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"TG-801A","index":0,"n_rows":83,"n_cols":13,"rows_kept":83,"merged":[[0,0,1,1],[0,2,1,3],[0,4,5,5],[0,6,5,8],[0,9,5,10],[2,0,3,1],[2,2,3,3],[4,0,5,1],[4,2,5,3],[6,0,6,10],[7,0,10,1],[7,2,10,2],[7,3,10,3],[7,4,10,4],[7,5,10,5],[7,6,7,10],[8,6,8,8],[8,9,8,10],[9,6,10,6],[9,7,10,7],[9,8,10,8],[9,9,10,9],[9,10,10,10],[11,0,11,1],[12,0,12,1],[13,0,13,1],[13,5,13,6],[14,1,14,2],[14,3,14,10],[15,1,15,2],[15,3,15,10],[16,1,16,2],[16,3,16,10],[17,1,17,2],[17,3,17,10],[18,1,18,2],[18,3,18,10],[19,1,19,2],[19,3,19,10],[20,0,22,0],[20,1,22,2],[20,4,20,9],[21,4,21,9],[22,4,22,9],[23,0,25,0],[23,1,25,2],[23,4,23,9],[24,4,24,9],[25,4,25,9],[26,0,28,0],[26,1,28,2],[26,4,26,9],[27,4,27,9],[28,4,28,9],[29,0,29,10],[30,1,30,2],[30,4,30,9],[31,1,31,2],[31,4,31,9],[32,1,32,2],[32,4,32,9],[33,1,33,2],[33,4,33,9],[34,1,34,2],[34,4,34,9],[35,1,35,2],[35,4,35,9],[36,1,36,2],[36,4,36,9],[37,1,37,2],[37,4,37,9],[38,1,38,2],[38,4,38,9],[39,1,39,2],[39,4,39,9],[40,1,40,2],[40,4,40,9],[41,1,41,2],[41,4,41,9],[42,0,42,10],[43,1,43,2],[43,4,43,9],[44,1,44,2],[44,4,44,9],[45,1,45,2],[45,4,45,9],[46,1,46,2],[46,4,46,9],[47,1,47,2],[47,4,47,9],[48,1,48,2],[48,4,48,6],[48,7,48,9],[49,1,49,2],[49,4,49,9],[50,1,50,2],[50,4,50,9],[51,1,51,2],[51,4,51,9],[52,0,54,0],[52,1,54,2],[52,3,54,3],[52,4,52,6],[52,7,52,9],[53,4,53,6],[53,7,53,9],[54,4,54,6],[54,7,54,9],[55,1,55,2],[55,4,55,9],[56,1,56,2],[56,4,56,9],[57,0,57,10],[58,1,58,2],[58,4,58,9],[59,1,59,2],[59,4,59,9],[60,1,60,2],[60,4,60,9],[61,1,61,2],[61,4,61,9],[62,0,62,10],[63,1,63,2],[63,4,63,9],[64,1,64,2],[64,4,64,9],[65,1,65,2],[65,4,65,9],[66,0,66,5],[66,6,69,10],[67,0,67,5],[68,0,68,5],[69,0,69,5],[70,0,70,10],[71,0,71,10],[72,0,72,10],[73,0,73,10],[74,0,74,10],[75,0,75,10],[76,0,76,10],[77,0,77,10],[78,0,78,10],[79,0,79,10],[80,0,80,10],[81,0,81,10],[82,0,82,10]]}
["Project",null,"CSIR BIDF",{"$nulls":6},{"$f":"\"Page \"&_xlfn.SHEET()&\" of \"&_xlfn.SHEETS()","v":"Page 1 of 3"}]
[]
["Document No.",null,"21050-CSI-IC-DAS-002"]
[]
["Location",null,"South Africa, KZN, Durban"]
[]
["Revision Status"]
["Rev No.",null,"Date","Prepared By","Revised Sheet","Revision","Approvals"]
[{"$nulls":6},"Checked By",null,null,"Approved By"]
[{"$nulls":6},"CI Engineer","Mechanical Engineer","Process Engineer","CI Snr Engineer","Process Snr Engineer"]
[]
["A",null,"09/07/2021","K Freese","ALL","Issued for Internal Review","M. Conradie",null,null,"P Le Grange"]
[]
[]
[1,"Description:",null,"Temperature Indicator"]
[2,"Reference P&ID:",null,"21050-CSI-PR-PID-012"]
[3,"Item Number:",null,"TG-801A"]
[4,"Quantity:",null,1]
[5,"Service:",null,"Local Temperature Indication"]
[6,"Measured Media:",{"$nulls":10},"Process to complete"]
[7,"Flowrate:",null,"min:",{"$nulls":6},"m³/h",null,"Mechanical To complete"]
[{"$nulls":3},"operating:",{"$nulls":6},"m³/h"]
[{"$nulls":3},"max:",{"$nulls":6},"m³/h"]
[8,"Temperature:",null,"design min:",{"$nulls":6},"oC"]
[{"$nulls":3},"operating:",{"$nulls":6},"oC"]
[{"$nulls":3},"design max:",{"$nulls":6},"oC"]
[9,"Pressure:",null,"design min:",{"$nulls":6},"kPa"]
[{"$nulls":3},"operating:",{"$nulls":6},"kPa"]
[{"$nulls":3},"design max:",{"$nulls":6},"kPa"]
["EC&I Information"]
[10,"IO Type:",null,null,"Mechanical"]
[11,"Display type and Range:",null,null,"Local Field Display only,  Gauge"]
[12,"Calibration Range:",null,null,"TBC",{"$nulls":5},"oC"]
[13,"Instrument Vendor Range:",null,null,"*",{"$nulls":5},"oC"]
[14,"Signal Type:",null,null,"N/A"]
[15,"Supply:",null,null,"N/A"]
[16,"Sensor Type/Temperature Element:",null,null,"*"]
[17,"Instrument Conduit Connection:",null,null,"N/A"]
[18,"Transmitter Connection To Temperature Element:",null,null,"N/A"]
[19,"Alarm and Trip Values:",null,null,"N/A"]
[20,"Electrical Components:",null,null,"N/A"]
[21,"Display/Gauge Range:",null,null," *See Item 12",{"$nulls":5},"oC"]
["Mechanical Information"]
[22,"Instrument Mounting and Orientation:"]
[23,"Instrument Mechanical Connection:"]
[24,"Enclosure Material and Construction:",null,null,"*"]
[25,"Components:"]
[26,"Process Line Size:",{"$nulls":8},"Inch"]
[27,"Thermowell Connections:",null,null,"Process Side Connection: ",null,null,"Instrument Side Connection: "]
[28,"Probe Stem Length:",null,null,"*"]
[29,"Probe Stem Diameter:",null,null,"*"]
[30,"Thermowell Type:",null,null,"*"]
[31,"Wave Calc Information:",null,null,"Process Flow Velocity:",{"$nulls":5},"m/s"]
[{"$nulls":4},"Process Density:",{"$nulls":5},"kg/m3"]
[{"$nulls":4},"Process Temperature:",{"$nulls":5},"oC"]
[32,"Thermowell Insertion Length:",null,null,"TBC",{"$nulls":5},"mm"]
[33,"Instrument Identification:",null,null,"Stainless Steel Tag Fixed to Instrument with Stainless Steel Wire \nID: TG-801A"]
["Rating Information"]
[34,"Design Code:"]
[35,"Accuracy Class:",{"$nulls":8},"%"]
[36,"Ingress Protection:"]
[37,"HAC Compliance:"]
["Vendor Information"]
[38,"Manufacturer:",null,null,"*"]
[39,"Model:",null,null,"*"]
[40,"PO Number:",null,null,"*"]
["1) *: Vendor To Specify",{"$nulls":5},"FAT to be included"]
["2) TBC: To Be Confirmed"]
["ALL REVISIONS WILL BE INDICATED BY GREY HIGHLIGHTING IN THE DOCUMENT BODY"]
["ALL ITEMS ON HOLD WILL BE INDICATED BY YELLOW HIGHLIGHTING IN THE DOCUMENT BODY"]
["QUALITY ASSURANCE PLAN OR QA/QC CHECKLIST"]
["MANUFACTURERS FUNCTIONAL TEST REPORT/ INSPECTION CERIFICATE "]
["MATERIAL CERTIFICATES"]
["HYDROSTATIC TEST CERTIFICATE IF APPLICABLE"]
["CERFITICATE OF CONFORMANCE "]
["DATASHEETS"]
["USER AND INSTALLATION MANUALS"]
["GENERAL ARRANGEMENT DRAWINGS"]
["HOOK-UP DRAWINGS"]
["ATEX AND I.A CERTIFICATES"]
["CALIBRATION CERTIFICATES"]
["SPARE PARTS LIST ( WHERE APPLICABLE)"]
["STAINLESS STEEL TAG"]

{"sheet":"TG-801B","index":1,"n_rows":83,"n_cols":13,"rows_kept":83,"merged":[[0,0,1,1],[0,2,1,3],[0,4,5,5],[0,6,5,8],[0,9,5,10],[2,0,3,1],[2,2,3,3],[4,0,5,1],[4,2,5,3],[6,0,6,10],[7,0,10,1],[7,2,10,2],[7,3,10,3],[7,4,10,4],[7,5,10,5],[7,6,7,10],[8,6,8,8],[8,9,8,10],[9,6,10,6],[9,7,10,7],[9,8,10,8],[9,9,10,9],[9,10,10,10],[11,0,11,1],[12,0,12,1],[13,0,13,1],[13,5,13,6],[14,1,14,2],[14,3,14,10],[15,1,15,2],[15,3,15,10],[16,1,16,2],[16,3,16,10],[17,1,17,2],[17,3,17,10],[18,1,18,2],[18,3,18,10],[19,1,19,2],[19,3,19,10],[20,0,22,0],[20,1,22,2],[20,4,20,9],[21,4,21,9],[22,4,22,9],[23,0,25,0],[23,1,25,2],[23,4,23,9],[24,4,24,9],[25,4,25,9],[26,0,28,0],[26,1,28,2],[26,4,26,9],[27,4,27,9],[28,4,28,9],[29,0,29,10],[30,1,30,2],[30,4,30,9],[31,1,31,2],[31,4,31,9],[32,1,32,2],[32,4,32,9],[33,1,33,2],[33,4,33,9],[34,1,34,2],[34,4,34,9],[35,1,35,2],[35,4,35,9],[36,1,36,2],[36,4,36,9],[37,1,37,2],[37,4,37,9],[38,1,38,2],[38,4,38,9],[39,1,39,2],[39,4,39,9],[40,1,40,2],[40,4,40,9],[41,1,41,2],[41,4,41,9],[42,0,42,10],[43,1,43,2],[43,4,43,9],[44,1,44,2],[44,4,44,9],[45,1,45,2],[45,4,45,9],[46,1,46,2],[46,4,46,9],[47,1,47,2],[47,4,47,9],[48,1,48,2],[48,4,48,6],[48,7,48,9],[49,1,49,2],[49,4,49,9],[50,1,50,2],[50,4,50,9],[51,1,51,2],[51,4,51,9],[52,0,54,0],[52,1,54,2],[52,3,54,3],[52,4,52,6],[52,7,52,9],[53,4,53,6],[53,7,53,9],[54,4,54,6],[54,7,54,9],[55,1,55,2],[55,4,55,9],[56,1,56,2],[56,4,56,9],[57,0,57,10],[58,1,58,2],[58,4,58,9],[59,1,59,2],[59,4,59,9],[60,1,60,2],[60,4,60,9],[61,1,61,2],[61,4,61,9],[62,0,62,10],[63,1,63,2],[63,4,63,9],[64,1,64,2],[64,4,64,9],[65,1,65,2],[65,4,65,9],[66,0,66,5],[66,6,69,10],[67,0,67,5],[68,0,68,5],[69,0,69,5],[70,0,70,10],[71,0,71,10],[72,0,72,10],[73,0,73,10],[74,0,74,10],[75,0,75,10],[76,0,76,10],[77,0,77,10],[78,0,78,10],[79,0,79,10],[80,0,80,10],[81,0,81,10],[82,0,82,10]]}
["Project",null,"CSIR BIDF",{"$nulls":6},{"$f":"\"Page \"&_xlfn.SHEET()&\" of \"&_xlfn.SHEETS()","v":"Page 2 of 3"}]
[]
["Document No.",null,"21050-CSI-IC-DAS-002"]
[]
["Location",null,"South Africa, KZN, Durban"]
[]
["Revision Status"]
["Rev No.",null,"Date","Prepared By","Revised Sheet","Revision","Approvals"]
[{"$nulls":6},"Checked By",null,null,"Approved By"]
[{"$nulls":6},"CI Engineer","Mechanical Engineer","Process Engineer","CI Snr Engineer","Process Snr Engineer"]
[]
["A",null,"09/07/2021","K Freese","ALL","Issued for Internal Review","M. Conradie",null,null,"P Le Grange"]
[]
[]
[1,"Description:",null,"Temperature Indicator"]
[2,"Reference P&ID:",null,"21050-CSI-PR-PID-012"]
[3,"Item Number:",null,"TG-801B"]
[4,"Quantity:",null,1]
[5,"Service:",null,"Local Temperature Indication"]
[6,"Measured Media:",{"$nulls":10},"Process to complete"]
[7,"Flowrate:",null,"min:",{"$nulls":6},"m³/h",null,"Mechanical To complete"]
[{"$nulls":3},"operating:",{"$nulls":6},"m³/h"]
[{"$nulls":3},"max:",{"$nulls":6},"m³/h"]
[8,"Temperature:",null,"design min:",{"$nulls":6},"oC"]
[{"$nulls":3},"operating:",{"$nulls":6},"oC"]
[{"$nulls":3},"design max:",{"$nulls":6},"oC"]
[9,"Pressure:",null,"design min:",{"$nulls":6},"kPa"]
[{"$nulls":3},"operating:",{"$nulls":6},"kPa"]
[{"$nulls":3},"design max:",{"$nulls":6},"kPa"]
["EC&I Information"]
[10,"IO Type:",null,null,"Mechanical"]
[11,"Display type and Range:",null,null,"Local Field Display only,  Gauge"]
[12,"Calibration Range:",null,null,"TBC",{"$nulls":5},"oC"]
[13,"Instrument Vendor Range:",null,null,"*",{"$nulls":5},"oC"]
[14,"Signal Type:",null,null,"N/A"]
[15,"Supply:",null,null,"N/A"]
[16,"Sensor Type/Temperature Element:",null,null,"*"]
[17,"Instrument Conduit Connection:",null,null,"N/A"]
[18,"Transmitter Connection To Temperature Element:",null,null,"N/A"]
[19,"Alarm and Trip Values:",null,null,"N/A"]
[20,"Electrical Components:",null,null,"N/A"]
[21,"Display/Gauge Range:",null,null," *See Item 12",{"$nulls":5},"oC"]
["Mechanical Information"]
[22,"Instrument Mounting and Orientation:"]
[23,"Instrument Mechanical Connection:"]
[24,"Enclosure Material and Construction:",null,null,"*"]
[25,"Components:"]
[26,"Process Line Size:",{"$nulls":8},"Inch"]
[27,"Thermowell Connections:",null,null,"Process Side Connection: ",null,null,"Instrument Side Connection: "]
[28,"Probe Stem Length:",null,null,"*"]
[29,"Probe Stem Diameter:",null,null,"*"]
[30,"Thermowell Type:",null,null,"*"]
[31,"Wave Calc Information:",null,null,"Process Flow Velocity:",{"$nulls":5},"m/s"]
[{"$nulls":4},"Process Density:",{"$nulls":5},"kg/m3"]
[{"$nulls":4},"Process Temperature:",{"$nulls":5},"oC"]
[32,"Thermowell Insertion Length:",null,null,"TBC",{"$nulls":5},"mm"]
[33,"Instrument Identification:",null,null,"Stainless Steel Tag Fixed to Instrument with Stainless Steel Wire \nID: TG-801B"]
["Rating Information"]
[34,"Design Code:"]
[35,"Accuracy Class:",{"$nulls":8},"%"]
[36,"Ingress Protection:"]
[37,"HAC Compliance:"]
["Vendor Information"]
[38,"Manufacturer:",null,null,"*"]
[39,"Model:",null,null,"*"]
[40,"PO Number:",null,null,"*"]
["1) *: Vendor To Specify",{"$nulls":5},"FAT to be included"]
["2) TBC: To Be Confirmed"]
["ALL REVISIONS WILL BE INDICATED BY GREY HIGHLIGHTING IN THE DOCUMENT BODY"]
["ALL ITEMS ON HOLD WILL BE INDICATED BY YELLOW HIGHLIGHTING IN THE DOCUMENT BODY"]
["QUALITY ASSURANCE PLAN OR QA/QC CHECKLIST"]
["MANUFACTURERS FUNCTIONAL TEST REPORT/ INSPECTION CERIFICATE "]
["MATERIAL CERTIFICATES"]
["HYDROSTATIC TEST CERTIFICATE IF APPLICABLE"]
["CERFITICATE OF CONFORMANCE "]
["DATASHEETS"]
["USER AND INSTALLATION MANUALS"]
["GENERAL ARRANGEMENT DRAWINGS"]
["HOOK-UP DRAWINGS"]
["ATEX AND I.A CERTIFICATES"]
["CALIBRATION CERTIFICATES"]
["SPARE PARTS LIST ( WHERE APPLICABLE)"]
["STAINLESS STEEL TAG"]

{"sheet":"TG-802","index":2,"n_rows":83,"n_cols":13,"rows_kept":83,"merged":[[0,0,1,1],[0,2,1,3],[0,4,5,5],[0,6,5,8],[0,9,5,10],[2,0,3,1],[2,2,3,3],[4,0,5,1],[4,2,5,3],[6,0,6,10],[7,0,10,1],[7,2,10,2],[7,3,10,3],[7,4,10,4],[7,5,10,5],[7,6,7,10],[8,6,8,8],[8,9,8,10],[9,6,10,6],[9,7,10,7],[9,8,10,8],[9,9,10,9],[9,10,10,10],[11,0,11,1],[12,0,12,1],[13,0,13,1],[13,5,13,6],[14,1,14,2],[14,3,14,10],[15,1,15,2],[15,3,15,10],[16,1,16,2],[16,3,16,10],[17,1,17,2],[17,3,17,10],[18,1,18,2],[18,3,18,10],[19,1,19,2],[19,3,19,10],[20,0,22,0],[20,1,22,2],[20,4,20,9],[21,4,21,9],[22,4,22,9],[23,0,25,0],[23,1,25,2],[23,4,23,9],[24,4,24,9],[25,4,25,9],[26,0,28,0],[26,1,28,2],[26,4,26,9],[27,4,27,9],[28,4,28,9],[29,0,29,10],[30,1,30,2],[30,4,30,9],[31,1,31,2],[31,4,31,9],[32,1,32,2],[32,4,32,9],[33,1,33,2],[33,4,33,9],[34,1,34,2],[34,4,34,9],[35,1,35,2],[35,4,35,9],[36,1,36,2],[36,4,36,9],[37,1,37,2],[37,4,37,9],[38,1,38,2],[38,4,38,9],[39,1,39,2],[39,4,39,9],[40,1,40,2],[40,4,40,9],[41,1,41,2],[41,4,41,9],[42,0,42,10],[43,1,43,2],[43,4,43,9],[44,1,44,2],[44,4,44,9],[45,1,45,2],[45,4,45,9],[46,1,46,2],[46,4,46,9],[47,1,47,2],[47,4,47,9],[48,1,48,2],[48,4,48,6],[48,7,48,9],[49,1,49,2],[49,4,49,9],[50,1,50,2],[50,4,50,9],[51,1,51,2],[51,4,51,9],[52,0,54,0],[52,1,54,2],[52,3,54,3],[52,4,52,6],[52,7,52,9],[53,4,53,6],[53,7,53,9],[54,4,54,6],[54,7,54,9],[55,1,55,2],[55,4,55,9],[56,1,56,2],[56,4,56,9],[57,0,57,10],[58,1,58,2],[58,4,58,9],[59,1,59,2],[59,4,59,9],[60,1,60,2],[60,4,60,9],[61,1,61,2],[61,4,61,9],[62,0,62,10],[63,1,63,2],[63,4,63,9],[64,1,64,2],[64,4,64,9],[65,1,65,2],[65,4,65,9],[66,0,66,5],[66,6,69,10],[67,0,67,5],[68,0,68,5],[69,0,69,5],[70,0,70,10],[71,0,71,10],[72,0,72,10],[73,0,73,10],[74,0,74,10],[75,0,75,10],[76,0,76,10],[77,0,77,10],[78,0,78,10],[79,0,79,10],[80,0,80,10],[81,0,81,10],[82,0,82,10]]}
["Project",null,"CSIR BIDF",{"$nulls":6},{"$f":"\"Page \"&_xlfn.SHEET()&\" of \"&_xlfn.SHEETS()","v":"Page 3 of 3"}]
[]
["Document No.",null,"21050-CSI-IC-DAS-002"]
[]
["Location",null,"South Africa, KZN, Durban"]
[]
["Revision Status"]
["Rev No.",null,"Date","Prepared By","Revised Sheet","Revision","Approvals"]
[{"$nulls":6},"Checked By",null,null,"Approved By"]
[{"$nulls":6},"CI Engineer","Mechanical Engineer","Process Engineer","CI Snr Engineer","Process Snr Engineer"]
[]
["A",null,"09/07/2021","K Freese","ALL","Issued for Internal Review","M. Conradie",null,null,"P Le Grange"]
[]
[]
[1,"Description:",null,"Temperature Indicator"]
[2,"Reference P&ID:",null,"21050-CSI-PR-PID-012"]
[3,"Item Number:",null,"TG-802"]
[4,"Quantity:",null,1]
[5,"Service:",null,"Local Temperature Indication"]
[6,"Measured Media:",{"$nulls":10},"Process to complete"]
[7,"Flowrate:",null,"min:",{"$nulls":6},"m³/h",null,"Mechanical To complete"]
[{"$nulls":3},"operating:",{"$nulls":6},"m³/h"]
[{"$nulls":3},"max:",{"$nulls":6},"m³/h"]
[8,"Temperature:",null,"design min:",{"$nulls":6},"oC"]
[{"$nulls":3},"operating:",{"$nulls":6},"oC"]
[{"$nulls":3},"design max:",{"$nulls":6},"oC"]
[9,"Pressure:",null,"design min:",{"$nulls":6},"kPa"]
[{"$nulls":3},"operating:",{"$nulls":6},"kPa"]
[{"$nulls":3},"design max:",{"$nulls":6},"kPa"]
["EC&I Information"]
[10,"IO Type:",null,null,"Mechanical"]
[11,"Display type and Range:",null,null,"Local Field Display only,  Gauge"]
[12,"Calibration Range:",null,null,"TBC",{"$nulls":5},"oC"]
[13,"Instrument Vendor Range:",null,null,"*",{"$nulls":5},"oC"]
[14,"Signal Type:",null,null,"N/A"]
[15,"Supply:",null,null,"N/A"]
[16,"Sensor Type/Temperature Element:",null,null,"*"]
[17,"Instrument Conduit Connection:",null,null,"N/A"]
[18,"Transmitter Connection To Temperature Element:",null,null,"N/A"]
[19,"Alarm and Trip Values:",null,null,"N/A"]
[20,"Electrical Components:",null,null,"N/A"]
[21,"Display/Gauge Range:",null,null," *See Item 12",{"$nulls":5},"oC"]
["Mechanical Information"]
[22,"Instrument Mounting and Orientation:"]
[23,"Instrument Mechanical Connection:"]
[24,"Enclosure Material and Construction:",null,null,"*"]
[25,"Components:"]
[26,"Process Line Size:",{"$nulls":8},"Inch"]
[27,"Thermowell Connections:",null,null,"Process Side Connection: ",null,null,"Instrument Side Connection: "]
[28,"Probe Stem Length:",null,null,"*"]
[29,"Probe Stem Diameter:",null,null,"*"]
[30,"Thermowell Type:",null,null,"*"]
[31,"Wave Calc Information:",null,null,"Process Flow Velocity:",{"$nulls":5},"m/s"]
[{"$nulls":4},"Process Density:",{"$nulls":5},"kg/m3"]
[{"$nulls":4},"Process Temperature:",{"$nulls":5},"oC"]
[32,"Thermowell Insertion Length:",null,null,"TBC",{"$nulls":5},"mm"]
[33,"Instrument Identification:",null,null,"Stainless Steel Tag Fixed to Instrument with Stainless Steel Wire \nID: TG-802"]
["Rating Information"]
[34,"Design Code:"]
[35,"Accuracy Class:",{"$nulls":8},"%"]
[36,"Ingress Protection:"]
[37,"HAC Compliance:"]
["Vendor Information"]
[38,"Manufacturer:",null,null,"*"]
[39,"Model:",null,null,"*"]
[40,"PO Number:",null,null,"*"]
["1) *: Vendor To Specify",{"$nulls":5},"FAT to be included"]
["2) TBC: To Be Confirmed"]
["ALL REVISIONS WILL BE INDICATED BY GREY HIGHLIGHTING IN THE DOCUMENT BODY"]
["ALL ITEMS ON HOLD WILL BE INDICATED BY YELLOW HIGHLIGHTING IN THE DOCUMENT BODY"]
["QUALITY ASSURANCE PLAN OR QA/QC CHECKLIST"]
["MANUFACTURERS FUNCTIONAL TEST REPORT/ INSPECTION CERIFICATE "]
["MATERIAL CERTIFICATES"]
["HYDROSTATIC TEST CERTIFICATE IF APPLICABLE"]
["CERFITICATE OF CONFORMANCE "]
["DATASHEETS"]
["USER AND INSTALLATION MANUALS"]
["GENERAL ARRANGEMENT DRAWINGS"]
["HOOK-UP DRAWINGS"]
["ATEX AND I.A CERTIFICATES"]
["CALIBRATION CERTIFICATES"]
["SPARE PARTS LIST ( WHERE APPLICABLE)"]
["STAINLESS STEEL TAG"]