{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["CSIR RFP No. 3597-03-11-2023"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"CSIR RFP No. 3597-03-11-2023","index":0,"n_rows":122,"n_cols":6,"rows_kept":122,"merged":[[113,1,113,2],[115,1,115,2],[117,1,117,2],[121,1,121,2]]}
[null,"NEW CAT LADDER INSTALLATIONS. \nPROVIDE COMPLETE PROJECT, ENCOMPASSING, DESIGNS, MANUFACTURING, INSTALLATION, CERTIFICATION, HAND OVER ACCOMPANIED BY ALL REGULATORY APPROVALS AND CERTIFICATIONS.","UNIT ","QUANTITY","RATE","AMOUNT"]
[]
[]
[null,"Notes "]
[null,"The Successful Contractor to Provide a Full Turnkey Project inclusive of: "]
[null,"Provision of Professional Services for the CAT LADDER Design, and municipal approvals including Chief Inspector of Department of Labour"]
[null,"Provision for the removal of existing structures, protection of existing building façades and associated elements"]
[null,"Provision for the manufacturing and installation of the HOT DIPPED GALVANISED Cat Ladders complete, to meet General safety regulations, 1986 and all related SANS codes for manufacturing and materials wrt hot dipped galvanised steel CAT ladders. "]
[null,"Provision of final certification and local authority approvals for regulatory compliance, inclusive of insurance requirements."]
[null,"Additional works are subject to prior approval of client."]
[]
[null,"Design Criteria"]
[null,"Design shall be in accordance with governing building codes and standards as applicable."]
[]
[null,"Performance requirements"]
[null,"Must meet the requirements set in the BS 5395:Part 3:1985 and meet the  requirement of the Occupational Health and Safety Act (Act85 of 1993) and the General safety regulations, Regulation 13A (6) of 1986"]
[]
[null,"View site"]
[null,"Before submitting his tender the tenderer shall visit the site and satisfy himself as to the nature and extent of the work to be done. No claim for any variations of the contract sum in respect of the nature and extent of the work or of inferior or damaged materials will be entertained"]
[]
[null,"NOTE: pricing is subject to compulsory pretender site inspections by all bidders"]
[]
[null,"SPECIFICATIONS"]
[]
[null,"Provide Turnkey services for the supply and installation of new Hot dipped Galvanised Steel Cat Ladders inclusive of all certifications and regulatory requirements"]
[]
[{"v":1,"d":"1 "},"Supply architectural impression for client final approval.","Item ",1,null,"R"]
[]
[{"v":2,"d":"2 "},"Design engineer's structural details for shop drawings\n (shop drawings to be completed by installers) note installation in separate BOQ","Item ",1,null,"R"]
[{"v":3,"d":"3 "},"Design, proposed methodology for the safe installation of the various cat ladders. ","Item ",1,null,"R"]
[]
[{"v":4,"d":"4 "},"Submit full construction programme, from concept to design stage inclusive of manufacturing and installation stage","Item ",1,null,"R"]
[]
[{"v":5,"d":"5 "},"Submission and approval process of all necessary motivations, proposals and plans to the local authorities for final approval and signoff of plans.","Item ",1,null,"R"]
[]
[{"v":6,"d":"6 "},"Provide Final sign-off by a practicing engineer","Item ",1,null,"R"]
[]
[{"v":7,"d":"7 "},"Supply and install New Hot dipped Galvanised Steel Cat Ladders per building as listed below"]
[null,"To meet all regulatory Design, Manufacturing, and Performance standards "]
[null,"In accordance with governing building codes and standards as applicable."]
[null,"Cat ladders to support their own weight and that of the user."]
[null,"Top rung of a ladder should be at the same level as the floor or landing at the head of the ladder."]
[null,"Allow for transition safety cage to the upper end of the ladder as per regulations."]
[]
[null,"Please Note: the lengths provided below is from the ground up to the transition height (floor or roof level) "]
[null,"Bidder to make allowance in the pricing for the extension height of the cage above transition level."]
[]
[{"v":8,"d":"8 "},"Supply and install Cat Ladders"]
[null,"Building 9"]
[null,"4m to roof ","Item",1,null,"R"]
[null,"2.5m to roof","Item",1,null,"R"]
[]
[null,"Building 13"]
[null,"4.5m to roof","Item",1,null,"R"]
[]
[null,"Building 14 A and B"]
[null,"4.5m to roof","Item",2,null,"R"]
[]
[null,"Building 14F"]
[null,"6.8m to roof","Item",1,null,"R"]
[]
[null,"Building 15"]
[null,"3.5m to roof","Item",1,null,"R"]
[]
[null,"Building 16"]
[null,"3m to roof","Item",1,null,"R"]
[]
[]
[null,"Building 18C"]
[null,"2.5m to roof","Item",1,null,"R"]
[null,"2.5m to roof","Item",1,null,"R"]
[]
[null,"Building 18a"]
[null,"5.6m to roof","Item",1,null,"R"]
[]
[null,"Building 21"]
[null,"4m to roof","Item",1,null,"R"]
[null,"4m to roof","Item",1,null,"R"]
[]
[null,"Building 43"]
[null,"Allow for 3.8meter ladders to roof","Item",7,null,"R"]
[]
[]
[{"v":10,"d":"10 "},"Supply and installation of Catwalk with balustrades"]
[null,"Building 9","Item",2,null,"R"]
[null,"3.5m length"]
[null,"3.5m length"]
[]
[{"v":11,"d":"11 "},"Supply and installation of Steel stairs to various roof levels"]
[null,"Building 10","Item",1,null,"R"]
[null,"Go over 1.5m heigh parapet wall"]
[null,"Building 11","Item",1,null,"R"]
[null,"Go over 1.5m heigh parapet wall"]
[null,"Building 12","Item",1,null,"R"]
[null,"Go over 1.5m heigh parapet wall"]
[null,"Building 16","Item",1,null,"R"]
[null,"Go over 1.5m heigh parapet wall"]
[null,"Building 43","Item",1,null,"R"]
[]
[]
[{"v":12,"d":"12 "},"Supply and installation of anchor bolts  (for Safety line hooks)"]
[null,"Building 43","Item",9,null,"R"]
[]
[{"v":13,"d":"13 "},"Allow for the removal and cart away of existing CAT Ladders ","Item",5,null,"R"]
[]
[]
[null,"Access and placement"]
[{"v":13,"d":"13 "},"Allow for hoisting and placement","Item",1,null,"R"]
[]
[null,"Safety"]
[{"v":14,"d":"14 "},"Allow for ALL HEATH and SAFETY requirements ","Item",1,null,"R"]
[]
[]
[null,"SUBTOTAL ALL ITEMS INCLUDED",{"$nulls":3},"R"]
[]
[null,"CONTINGENCY AMOUNT ",null,{"v":0.1,"d":"10%"},null,"R"]
[]
[null,"SUBTOTAL",{"$nulls":3},"R"]
[]
[null,null,"VAT",{"v":0.15,"d":"15%"},null,"R"]
[]
[null,"TOTAL PRICE INCLUSIVE OF VAT",{"$nulls":3},"R"]